MATLAB File Help: wrsamp | View code for wrsamp | WFDB Contents

wrsamp

    function varargout=wrsamp(varargin)

     wrsamp(tm,data,fileName,Fs,gain,format)

        Wrapper to WFDB WRSAMP:
             http://www.physionet.org/physiotools/wag/wrsamp-1.htm

     Writes data into a WFDB annotation file. The file will be saved at the
     current directory (if the record is in the current directory) or, if a using
     a PhysioNet web record , a subdirectory in the current directory, with
     the relative path determined by recordName. The files will have the same
     name is the recordName but with a 'annotator' extension. You can use RDANN to
     verify that the write was completed sucessfully (see example below). For
     detailed information on the parameters described below, please see:
     http://www.physionet.org/physiotools/wag/header-5.htm

     Required Parameters:

     tm
           Nx1 vector of integers representing sample index.

     data
           NxM vector of integers (M channels) that will be written to file.

     fileName

           String specifying the file name. WRSAMP will write the signal file in
           the current directory as "fileName.dat", and create a header file in the
           current directory "fileName.hea" for the specified record.

     Optional Parameters:

     Fs
           A 1x1 double specifying the sampling frequency (in samples per second per
           signal) for the output signals (default: 250). It affects the output header
           file only. This option has no effect on the output signal file, which
           contains one sample per signal for each line of input.

     gain
           A 1x1 or Mx1 vector of doubles specifying gain value in A/D units per millivolt
           for the output signals (default: 200).  This option the output header file only.
           This option has no effect on the output signal file.

     format
           String specifying the signal's default format (default: "16"). For
           information on the available WFDB formats please see:
           http://www.physionet.org/physiotools/wag/signal-5.htm

    %Example-
    %Read signal in raw units
    [tm, signal]=rdsamp('challenge/2013/set-a/a01',[],[],[],1);
    [siginfo,Fs]=wfdbdesc('challenge/2013/set-a/a01');
    %Write a copy to file
    wrsamp(tm,signal(:,1),'a01Copy',Fs(1),200,siginfo(1).Format)
    %Check that the signals match
    [tm, signalCopy]=rdsamp('a01Copy',[],[],[],1);
    err=sum(signalCopy ~= signal(:,1))

     Written by Ikaro Silva, 2013
     Last Modified: -
     Since 0.0.1

     See also rdsamp, wfdbdesc