MATLAB File Help: wfdb2mat | View code for wfdb2mat | WFDB Contents

wfdb2mat

    function varargout=wfdb2mat(varargin)

     wfdm2mat(recordName,signaList,N,N0)

        Wrapper to WFDB WFDB2MAT:
             http://physionet.org/physiotools/wag/wfdb2m-1.htm

     Converts a WFDB-compatible signal file to MATLAB/Octave *.mat file.
     The output files are recordNamem.mat and recordNamem.hea. The standard output of
     WFDB2MAT will be saved in a file recordNamem.info.

     Required Parameters:

     recorName
           String specifying the name of the record in the WFDB path or
           in the current directory.

     Optional Parameters are:

     signalList
           A Mx1 array of integers. Read only the signals (columns)
           named in the signalList (default: read all signals).
     N
           A 1x1 integer specifying the sample number at which to stop reading the
           record file (default read all the samples = N).
     N0
           A 1x1 integer specifying the sample number at which to start reading the
           record file (default 1 = first sample).

     NOTE:
           You can use the WFDB2MAT command in order to convert the record data into a *.mat file,
           which can then be loaded into MATLAB/Octave's workspace using the LOAD command.
           This sequence of procedures is quicker (by several orders of magnitude) than calling RDSAMP.
           This will load the signal data in raw units (use RDMAT to load the signal in physical units).

     Written by Ikaro Silva, 2014
     Last Modified: September 15, 2014
     Version 0.1

     Since 0.9.7

     %Example:
     wfdb2mat('mitdb/200')
     [tm,signal,Fs,labels]=rdmat('200m.mat');

     See also RDSAMP, RDMAT